RED TEXT INDICATES CITATION COULD NOT BE FOUND VIA WEB SEARCH

* Y. Huang, A. Shrivastava, L. Barnes, and B. H. Calhoun, “A Design and Theoretical Analysis of a 145 mV to 1.2 V Single-Ended Level Converter Circuit for Ultra-Low Power Low Voltage ICs,” J. Low Power Electron. Appl. (JLPEA), Vol. 6, No. 3, 2016.
* D. Akella Kamakshi, A. Shrivastava, and B. H. Calhoun, “A 0.2 V, 23 nW CMOS Temperature Sensor for Ultra-Low-Power IoT Applications,” J. Low Power Electron. Appl. (JLPEA), Vol. 6, No. 2, 2016.
* F. Yahya, H. Patel, J. Boley, A. Banerjee, and B. H. Calhoun, “A Sub-threshold 8T SRAM Macro with 12.29nW/KB Standby Power and 6.24 pJ/access for Battery-Less IoT SoCs,” J. Low Power Electron. Appl. (JLPEA), Vol. 6, No. 2, 2016.
* D. Akella, A. Shrivastava, C. Duan, and B. H. Calhoun, “A 36nW, 7 ppm/oC Fully On-Chip Clock Source System for Ultra-Low Power Applications,” Journal of Low Power Electronics and Applications (JLPEA), Vol. 6, No. 2, 2016.
* A. Roy, A. Klinefelter, F. B. Yahya, X. Chen, P. Gonzalez, D. Akella, J. Boley, K. Craig, M. Faisal, S. Oh, N. E. Roberts, Y. Shakhsheer, A. Shrivastava, D. Vasudevan, D. D. Wentzloff, and B. H. Calhoun, “A 6.45μW Self-Powered SoC with Integrated Energy-Harvesting Power Management and ULP Asymmetric Radios for Portable Biomedical Systems,” Transactions on Biomedical Circuits and Systems (TBioCAS), 2015.
* A. Shrivastava, D. Akella, and B. H. Calhoun, “A 1.5nW, 32.768kHz XTAL Oscillator Operational from 0.3V Supply,” IEEE Journal of Solid-State Circuits (JSSC), 2015.
* Shrivastava, N. E. Roberts, O. U. Khan, D. D. Wentzloff, and B. H. Calhoun, “A 10mV-Input Boost Converter with Inductor Peak Current Control and Zero Detection for Thermoelectric and Solar Energy Harvesting with 220mV Cold-Start and -14.5dBm, 915MHz RF Kick-Start,” IEEE Journal of Solid-State Circuits (JSSC), Vol. 50, No. 8, pages 1820-1832, August 2015.
* V. Misra, A. Bozkurt, B. Calhoun, T. Jackson, J. Jur, J. Lach, B. Lee, J. Muth, O. Oralkan, M. Ozturk, S. Trolier-McKinstry, D. Vashaee, D. Wentzloff, and Y. Zhu, “Flexible Technologies for Self-Powered Wearable Health and Environmental Sensing,” Proceedings of the IEEE, Vol. 103, No. 4, pages 665-681, April 2015.
* P. Long, J. Z. Huang, M. Povolotskyi, D. Verreck, J. Charles, T. Kubis, G. Klimeck, M. J.W. Rodwell, and B. H. Calhoun, “A Tunnel FET Design for High-Current, 120 mV Operation,” IEDM, 2016. (accepted)
* H. N. Patel, A. Roy, F. B. Yahya, N. Liu, K. Kumeno, M. Yasuda, A. Harada, T. Ema, B. H. Calhoun, “A 55nm Ultra Low Leakage Deeply Depleted Channel Technology Optimized for Energy Minimization in Subthreshold SRAM and Logic,” European Solid State Circuits Conference (ESSCIRC), 2016.
* N. Liu and B. H. Calhoun, “Design Optimization of Register File Throughput and Energy using a Virtual Prototyping (ViPro) Tool,” ISVLSI, 2016.
* D. Kamakshi, M. Fojtik, B. Khailany, S. Kudva, Y. Zhou, and B. H. Calhoun, “Modeling and Analysis of Power Supply Noise Tolerance with Fine-grained GALS Adaptive Clocks,” ASYNC, 2016. (Best Paper Award Nominee)
* A. Roy and B. H. Calhoun, “Exploring circuit robustness to power supply variation in low-voltage latch and register-based digital systems,” International Symposium on Circuits and Systems (ISCAS), 2016.
* A. Roy, P. Grossman, S. Vitale, and B. H. Calhoun, “A 1.3μW, 5pJ/cycle sub-threshold MSP430 processor in 90nm xLP FDSOI for energy-efficient IoT applications,” International Symposium on Quality Electronic Design (ISQED), 2016.
* H. Patel, F. Yahya, and B. H. Calhoun, “Optimizing SRAM Bitcell Reliability and Energy for IoT Applications,” International Symposium on Quality Electronic Design (ISQED), 2016.
* H. Patel, F. Yahya, and B. H. Calhoun, “Improving Reliability and Energy Requirements of Memory in Body Sensor Networks,” VLSI Design, 2016. **(accepted)**
* D. Akella, A. Shrivastava, and B. H. Calhoun, “A 23 nW CMOS ultra-Low Power Temperature Sensor Operational from 0.2 V,” IEEE SOI-3D-Subthreshold Microelectronics Technology Unified Conference (S3S), 2015.
* Y. Huang, A. Shrivastava, and B. H. Calhoun, “A 145mV to 1.2V Single Ended Level Converter Circuit for Ultra-Low Power Low Voltage ICs,” IEEE SOI-3D-Subthreshold Microelectronics Technology Unified Conference (S3S), 2015.
* A. Banerjee, J. Breiholz, and B. H. Calhoun, “A 130nm Canary SRAM for SRAM Dynamic Write VMIN Tracking across Voltage, Frequency, and Temperature Variations”, IEEE Custom Integrated Circuits Conference (CICC), 2015.
* J. Boley and B. H. Calhoun, “Stack Based Sense Amplifier Designs for Reducing Input-Referred Offset,” ISQED, 2015. (Best Paper Award Nominee)
* A. Klinefelter, J. Ryan, J. Tschanz, and B. H. Calhoun, “Error-Energy Analysis of Hardware Logarithmic Approximation Methods for Low Power Applications,” ISCAS, pages 2361-2364, 2015.
* C. J. Lukas and B. H. Calhoun, “A 0.38 pJ/bit 1.24 nW Chip-to-Chip Serial Link for Ultra-Low Power Systems,” ISCAS, pages 2860-2863, 2015.
* A. Klinefelter, N. Roberts, Y. Shakhsheer, P. Gonzalez, A. Shrivastava, A. Roy, K. Craig, M. Faisal, J. Boley, S. Oh, Y. Zhang, D. Akella, D. D. Wentzloff, B. H. Calhoun, “A 6.45 μW Self-Powered IoT SoC with Integrated Energy-Harvesting Power Management and ULP Asymmetric Radios,” IEEE International Solid-State Circuits Conference, 2015.
* **J. Gong, D. Fan, L. Lopez Ruiz, J. Lach, “Profiling, Modeling, and Predicting Energy Harvesting for Self-Powered Body Sensor Platforms,” BSN, 2016**
* S. Russell, Y. Zhuang, J. Gong, D.C. Kerrigan, B.C. Bennett, J. Lach, “Gait Tracker Shoe for Accurate Step-by-Step Determination of Gait Parameters,” BSN, 2016
* S.R. Dandu, M.M. Engelhard, M.D. Goldman, J. Lach, “,” BSN, 2016 Determining Physiological Significance of Inertial Gait Features in Multiple Sclerosis
* D. Fan, J. Gong, J. Lach, “Eating Gestures Detection by Tracking Finger Motion,” Wireless Health, 2016
* J. Gong, M.D. Goldman, J. Lach, “DeepMotion: A Deep Convolutional Neural Network on Inertial Body Sensors for Gait Assessment in Multiple Sclerosis,” Wireless Health, 2016 (**Best Paper Award Finalist**)
* M.M. Engelhard, J. Lach, M.D. Goldman, S.D. Patek, “Adaptive Symptom Reporting for Mobile Patient-Reported Disability Assessment,” Wireless Health, 2016 (**Best Paper Award Finalist**)
* J. Gong, P. Asare, Y. Qi, J. Lach, “Piecewise Linear Dynamical Model for Action Clustering from Real-World Deployments of Inertial Body Sensors,” IEEE Transactions on Affective Computing, April 2016
* M.M. Engelhard, S.R. Dandu, S.D. Patek, J. Lach, M.D. Goldman, “Quantifying Six-Minute Walk Induced Gait Deterioration with Inertial Sensors in Multiple Sclerosis Subjects,” Gait & Posture, July 2016
* J. Gong, Y. Qi, M.D. Goldman, J. Lach, “Causality Analysis of Inertial Body Sensors for Multiple Sclerosis Diagnostic Enhancement,” IEEE Journal of Biomedical and Health Informatics, September 2016
* S. Chen, J. Lach, B. Lo, G.-Z. Yang, “Towards Pervasive Gait Analysis with Wearable Sensors: A Systematic Review,” Journal of Biomedical and Health Informatics, in press
* A. Dirafzoon, N. Lokare and E. Lobaton, “Action Classification from Motion Capture Data using Topological Data Analysis,” IEEE Global Conf. on Signal and Information Processing (GlobalSIP), 2016.
* N. Lokare, D. Benavides, S. Juneja and E. Lobaton, “Hierarchical Activity Clustering Analysis for Robust Graphical Structure Recovery,” IEEE Global Conf. on Signal and Information Processing (GlobalSIP), 2016.
* N. Lokare, L. Gonzalez and E. Lobaton, “Comparing the Effect of Muscle Activation in Wearable Devices using Wet and Textile Electrodes,” IEEE Engineering in Medicine and Biology Conference (EMBC), 2016.
* H. G. Yeo, X. K. Ma, C. D. Rahn, and S. Trolier-McKinstry, “Efficient Piezoelectric Energy Harvesters Utilizing (001) Textured Bimorph PZT Films on Flexible Metal Foils,” *Advanced Functional Materials* (2016).
* X. K. Ma, S. Trolier-McKinstry, and C. D. Rahn, “Piezoelectric compliant mechanism energy harvesters under large base excitations,” *Smart Materials and Structures* 25 (9) 095023 (2016).
* X. K. Ma, A. Wilson, S. Trolier-McKinstry, and C. D. Rahn, “Efficient Energy Harvesting Using Piezoelectric Compliant Mechanisms: Theory and Experiment,” *Journal of Vibration and Acoustics-TRANSACTIONS ASME* 138 (2) 021005 (2016).
* X. K. Ma, H. G. Yeo, C. D. Rahn, and S. Trolier-McKinstry, “Efficient and Sensitive Energy Harvesting Using Piezoelectric MEMS Compliant Mechanisms,” *International Design Engineering Technical Conferences and Computers and Information in Engineering Conference, 2015,* 8, V008T13A042 (2016).
* Francisco Suarez , Dishit P. Parekh , Collin Ladd , Daryoosh Vashaee, Michael D. Dickey and Mehmet C. Ozturk, “Wearable thermoelectric Generator using bulk legs and liquid metal interconnects”
* Wearable thermoelectric generators for human body heat harvesting, Melissa Hyland, Haywood Hunter, Jie Liu, Elena Veety, Daryoosh Vashaee, Applied Energy 182 (2016) 518–524 (Featured in media and top story of NSF Science360 news)
* Classification of Valleytronics in Thermoelectricity, Payam Norouzzadeh and Daryoosh Vashaee, Scientific Reports 6, Article number: 22724 (2016) doi:10.1038/srep22724.
* Designing Thermoelectric Generators for Self-Powered Wearable Electronics, Francisco Suarez, Amin Nozariasbmarz, Daryoosh Vashaee and Mehmet Cevdet Ozturk, Energy & Environmental Science, 9, 2099-2113 (2016)
* Agrawal, R. , Chen, C., Dages, S., and Wang, C., A High Energy 3V Lithium-Ion Capacitor Synthesized via Electrostatic Spray Deposition, *Advanced Materials Letters* (In Press)
* Yuan, J., Chen, C., Hao, Y., Zhang, X., Zou, B., Agrawal, R., Wang, C., Yu, H., Zhu, X., Yu, Y., Xiong, Z., Luo, Y., Li, H., Xie, Y., SnO2/polypyrrole hollow spheres with improved cycle stability as lithium-ion battery anodes, Journal of Alloys and Compounds, 2017, 691, 34-39, doi: 10.1016/j.jallcom.2016.08.229.
* Agrawal, R., Chen, C., Dages, S., and Wang, C., Lithium-Ion Capacitor Based on Electrodes Constructed Via Electrostatic Spray Deposition, ECS Trans. 2016 volume 72, issue 8, 45-53. doi: 10.1149/07208.0045ecst
* Agrawal, R., Chen, C., and Wang, C., Electrostatic Spray Deposition based lithium-ion capacitor, *Proc. SPIE 9865, Energy Harvesting and Storage: Materials, Devices, and Applications VII, 986508* (17 May 2016) doi: 10.1117/12.2228899
* Chen, C., Agrawal, R., Wang, C. - Electrostatic spray deposition of Li4Ti5O12 based anode with enhanced rate capability and energy density for Lithium-ion batteries, *Proc. SPIE 9865, Energy Harvesting and Storage: Materials, Devices, and Applications VII, 986507* (17 May 2016) doi: 10.1117/12.2228905
* Chunhui Chen, Richa Agrawal, Chunlei Wang - *High performance Li4Ti5O12/Si composites as Li-ion battery anodes* – *Nanomaterials,* 2015, 5(3), 1469-1480; doi:10.3390/nano5031469
* **Xue, T., Roundy, S., 2016. “On Magnetic Plucking Configurations for Frequency Up-Converting Mechanical Energy Harvesters”, *Sensors and Actuators A: Physical*. [Under Review]**
* **Xue, T., Kakkar, S. Lin, Q., and Roundy, S. 2016. “Characterization of Micro-Generators Embedded in Commercial-Off-the-Shelf Watches for Wearable Energy Harvesting”, *SPIE Smart Structures and Materials+ Nondestructive Evaluation and Health Monitoring*, pp. 98010O-98010O. International Society for Optics and Photonics, 2016.**
* **Xue, T., and Roundy, S. 2015. “Analysis of Magnetic Plucking Configurations for Frequency Up-Converting Harvesters”, *Journal of Physics: Conference Series.* Vol. 660. N. 1. IOP Publishing, 2015.**
* **Xue, T., Ma, X., Rahn, C., and Roundy, S., 2014. "Analysis of Upper Bound Power Output for a Wrist-Worn Rotational Energy Harvester from Real-World Measured Inputs." Journal of Physics: Conference Series. Vol. 557. No. 1. IOP Publishing, 2014.**